| Construction Notes Manager for AutoCAD |
| CNM "Construction Notes Manager" Tutorial - Section Three |
| Introduction: Section One: INSTALLING CNM ∓SETUP Section Two: TUTORIALSETUP Section Three: EDITING PROJECT NOTES Section Four: INSERTING "BUBBLE NOTES" Section Five: EDITING BUBBLE NOTES Section Six: RUNNING "NOTES MANAGER Section Seven: PHASED CONSTRUCTION NOTES Section Eight: QUANTITY TAKE-OFF SectionNine: CNM Editor Configuration Section Ten: Customizing CNM SectionEleven: Video Files |
| 3.0 - EDITING PROJECTNOTES |
| Under the pull down menu "CNM" click on "Edit Project Notes" orpick the icon on the toolbar. |  |
|  |  | Edit Notes Icon |
| The program creates and uses a file called "Consnot.txt" which is the master notes file foradrawing or set of drawings that useskey notes. This file is simply a text file, but is formatted in such a way as to be used in the CNM editor. A sample "Constnot.txt" file is shown below. |
| Once you click on theEdit Project Notes button, if there is not an existing "Consnot.txt" file in your project folder, the program willpromptyou to select the location you wish to keep the current project notes. The program is flexible in that you may create and select the master notes file from a library, or you may have themaster notesfile reside in your project folder. |
| In this example, the consnot.txt file is set to the"CNM Tutorial" folder. |
| Note: Another way to bring this file into your project directory is simply to copy and paste using windows explorer. If you've created a template to use on subsequent projects, then make a backup of the default consnot.txt file (such as consnot.bk1) and copy your template over the default consnot.txt file. Alternately, just make a library of the consnot.txt files and copy and paste them into your working project directory as needed. |
| Once you select where you wish the constnot file to reside, the program will open the editor. The following picture shows what the editor looks like, without any notes |
| Since there are no active note files, select "Import Notes from Library" from the File pulldown menu as shown below |
|  | The "Export Notes to Library" allows you to save a notes file to the library as the name implies |
|  | "Change Library Path" allows you to change to another path for importing the notes file. This could be real helpful in setting up CAD standards |
| Select the consnot.txt file you wish to use for your particular project. For this tutorial select the one as shown below. Once highlighted click on the import button. |
| The imported file will add in the notes as shown below. Notice the tabs at the top. There is a tab for circle notes, hexagon notes, box notes, pentagon notes, etc. Also note how the information to be used is divided into columns. The "Not Used" column is simply a way for the CAD operator to know quickly whether or not a note is to be used. Also, the program will ignorethisconstruction note. The "Bubble #" column corresponds with the bubble note number as used in the drawing. The "Description" column is the actual construction note verbage as desired for the drawing. The "Unit" column indicates what type of unit is to be used for the note. The "Type" column tells the program what option to use when counting quantities. The only fields that are required are the "Bubble #" , the "Description" and the "Type". The other information can be optional as needed for your drawing. |
| In order to create new notes in the file, simply click on the "Insert" button and type in each field as needed. The note will be inserted below any "highlighted" row. In order to add a note to the bottom, simply click on the last note so that it is highlighted before hitting "Insert". As shown below in the next two figures, afewnotes have been inserted showing off a few of the options of each of the columns. Noticehow the note can word wrap in the description field. Also, for the Unit and Type you can select one of the predefined selections or type it in for a more customplan. |