;HawsEDC stock version 1.0, 1999
;Revised 2008 to reflect National CAD Standard/AIA conventions
;
;LAYERS.DAT
;By Thomas Gail Haws
;
;Layers defaults file for lisp routines
;
;Use this file to change CNM/HawsEDC layer names, colors, or linetypes.
;
;The commands depend on the lines in this file.
;If you remove any of the lines in this file or modify the key names,
;it may cause program instability, or in the best case, the current layer
;will be used benignly.
;
("NOTESEXP"     "C-ANNO-HCNM-TABL-EXPT"           "m"   "")         ;Key Notes table
("NOTESIMP"     "C-ANNO-HCNM-TABL-IMPT"           "m"   "")         ;Imported Key Notes table (from another drawing)
("NOTESKEYGRID" "C-ANNO-HCNM-TABL-GRID"           "13"  "")         ;Key Notes table grid
("NOTESKEYQTYS" "C-ANNO-HCNM-TABL-QTTY"           "2"   "")         ;Key Notes table quantities attributes.
("NOTESLDR"     "C-ANNO-HCNM-BUBL"                "m"   "")         ;Bubble notes, BOX, CIR, DIA, ELL, HEX, PEN, etc.
("NOTESTAL"     "C-ANNO-HCNM-TABL-TOTL"           "m"   "")         ;Quantity Take-off table
("NOTESNOPLOT"  "C-ANNO-HCNM-NPLT"                "252" "")         ;CNM layer to hide attributes on.
("0"            "0"                               ""    "")         ;Layer to insert multilayer or explode blocks on (usually"0")
("ANNOMISC"     "C-ANNO"                          "m"   "")         ;Misc annotation objects and INSBLK commands
("BB"           "C-ANNO-BUBL"                     ""    "")         ;BB command
("BERM"         "C-TOPO-BERM"                     "2"   "")         ;BERM command
("BWLDR"        "C-ANNO-LEAD"                     "1"   "")         ;BW command
("CLOUD"        "C-ANNO-CLOU"                     "3"   "")         ;CLD command revision clouds
("CONTLBL"      "C-TOPO-IDEN"                     ""    "")         ;CONTXT command
("IB-DELTA"     "C-ANNO-REVS"                     "2"   "")         ;DELTA command
("IB-SEC"       "C-ANNO-SECN"                     "2"   "")         ;SEC? commands
("DIM"          "C-ANNO-DIMS"                     "2"   "")         ;STDIM command
("DRIVEWAY"     "C-ROAD-DWAY"                     "6"   "")         ;DW command driveway
("DRIVEWAYTX"   "C-ROAD-DWAY-CL"                  "2"   "CENTER2")  ;DW command driveway centerline and text
("PCB"          "C-ANNO-PROF-STRM-INLT"           "8"   "")         ;PROCB command profile catch basin
("PEL"          "C-ANNO-PROF-UTIL-ELPS"           "8"   "")         ;PROE command profile pipe ellipse
("PELEVLBL"     "C-ANNO-PROF-ELEV"                "3"   "")         ;ELV command profile side elevations
("PGB"          "C-ANNO-PROF-TEXT"                ""    "")         ;GRB command grade break
("PGC"          "C-ANNO-PROF-TEXT"                ""    "")         ;GRC command grade change
("PLDR"         "C-ANNO-PROF-TEXT"                "2"   "")         ;PLDR command profile label leader
("PMH"          "C-ANNO-PROF-MHOL"                "8"   "")         ;PROMH command profile manhole
("PROCB"        "C-ANNO-PPRO-STRM-CBAS"           "8"   "")         ;PRO command profile catch basin
("PRODIM"       "C-ANNO-PPRO-DIMS"                "2"   "")         ;PRO command dimensions
("PROEL"        "C-ANNO-PPRO-UTIL-ELPS"           "4"   "")         ;PRO command profile pipe ellipse
("PROELTX"      "C-ANNO-PPRO-UTIL-ELPS-TEXT"      "2"   "")         ;PRO command profile pipe ellipse text
("PROEXMID"     "EXST-"                           "9"   "HIDDEN")   ;PRO command existing layers flag (goes between prefix and root)
("PROLINE"      "C-ANNO-PPRO-LINE"                ""    "")         ;PRO command line only profile
("PROMH"        "C-ANNO-PPRO-MH"                  "8"   "")         ;PRO command profile manhole
("PROPNT"       "DEFPOINTS"                       ""    "")         ;PRO command profile point circle
("PROPRE"       "C-ANNO-PPRO-"                    "4"   "")         ;PRO command layer prefix (for building layer names)
("PROSD"        "C-ANNO-PPRO-STRM"                "3"   "")         ;PRO command SD profile lines
("PROSEW"       "C-ANNO-PPRO-SSWR"                "4"   "")         ;PRO command SEW profile lines
("PROSTRT"      "C-ANNO-PPRO-CG"                  "7"   "")         ;PRO command street profile lines
("PROTXSUF"     "-TEXT"                           "2"   "")         ;PRO command text layer suffix (for building layer names)
("PROWAT"       "C-ANNO-PPRO-WATR"                "7"   "")         ;PRO command WAT profile lines
("PROXCB"       "C-ANNO-PPRO-STRM-CBAS-E"         "9"   "")         ;PRO command profile existing catch basin
("PROXDIM"      "C-ANNO-PPRO-DIMS-E"              "9"   "HIDDEN")   ;PRO command existing dimensions
("PROXEL"       "C-ANNO-PPRO-ELPS-E"              "9"   "HIDDEN")   ;PRO command profile existing pipe ellipse
("PROXELTX"     "C-ANNO-PPRO-ELPS-TEXT-E"         "9"   "")         ;PRO command profile existing pipe ellipse text
("PROXLINE"     "C-ANNO-PPRO-LINE-E"                   "9"   "HIDDEN")   ;PRO command existing line only profile
("PROXMH"       "C-ANNO-PPRO-MHOL-E"                   "9"   "")         ;PRO command profile existing manhole
("PROXSTRT"     "C-ANNO-PPRO-CURB-E"                   "9"   "HIDDEN")   ;PRO command existing street profile lines
("PROXTXSUF"    "-TEXT"                           "9"   "")         ;PRO command existing text layer suffix (for building layer names)
("PSTALBL"      "C-PROF-STAT"                     "3"   "")         ;STALABEL command profile bottom stations
("PSUP"         "C-PROF-SUPP"                     "1"   "")         ;PROSUP command pipe support
("PXCB"         "C-PROF-CBAS-E"                   "9"   "")         ;PROCB command profile existing catch basin
("PXEL"         "C-PROF-ELPS-E"                   "9"   "")         ;PROE command profile pipe ellipse
("PXLDR"        "C-PROF-TEXT-E"                   "9"   "")         ;PLDR command profile existing label leader
("PXMH"         "C-PROF-MHOL-E"                   "9"   "")         ;PROMH command profile existing manhole
("SEWTAP"       "C-SSWR-TAP"                      "8"   "")         ;TAP command sewer taps
("SEWTAPTX"     "C-SSWR-TAP-DIM"                  "5"   "")         ;TAP command sewer tap text
("SHTMVW"       "DEFPOINTS"                       ""    "")         ;SHEET command paper space viewports
("STDIM"        "C-ANNO-ROAD-DIMS"                "2"   "")         ;STDIM command
("TCGLDR"       "C-ANNO-ELEV"                     "2"   "")         ;TCG with leader command
("UTCATVOD"     "C-CATV-OD~~"                     "1"   "")         ;UT command thick CATV OD lines
("UTCATVPL"     "C-CATV-INNR"                     "9"   "UTILPL")   ;UT command thick CATV polylines
("UTCATVSNG"    "C-CATV"                          "1"   "")         ;UT command single line CATV lines
("UTELECOD"     "C-ELEC-OD~~"                     "3"   "")         ;UT command thick ELEC OD lines
("UTELECPL"     "C-ELEC-INNR"                     "9"   "UTILPL")   ;UT command thick ELEC polylines
("UTELECSNG"    "C-ELEC"                          "3"   "BLDG")     ;UT command single line ELEC lines
("UTGASOD"      "C-NGAS-OD~~"                     "5"   "")         ;UT command thick GAS OD lines
("UTGASPL"      "C-NGAS-INNR"                     "9"   "UTILPL")   ;UT command thick GAS polylines
("UTGASSNG"     "C-NGAS"                          "5"   "PHANTOM2") ;UT command single line GAS lines
("UTIRROD"      "C-IRRG-OD~~"                     "2"   "")         ;UT command thick IRR OD lines
("UTIRRPL"      "C-IRRG-INNR"                     "9"   "UTILPL")   ;UT command thick IRR polylines
("UTIRRSNG"     "C-IRRG"                          "2"   "HIDDEN")   ;UT command single line IRR lines
("UTSDOD"       "C-STRM-OD~~"                     "1"   "")         ;UT command thick SD OD lines
("UTSDPL"       "C-STRM-INNR"                     "9"   "UTILPL")   ;UT command thick SD line polylines
("UTSDSNG"      "C-STRM"                          "1"   "HIDDEN")   ;UT command single SD lines
("UTSEWOD"      "C-SSWR-OD~~"                     "4"   "")         ;UT command thick sewer OD lines
("UTSEWPL"      "C-SSWR-INNR"                     "9"   "UTILPL")   ;UT command thick sewer polylines
("UTSEWSNG"     "C-SSWR"                          "4"   "")         ;UT command single line sewer lines
("UTTELOD"      "C-TELE-OD~~"                     "5"   "BLDG")     ;UT command thick TEL OD lines
("UTTELPL"      "C-TELE-INNR"                     "9"   "UTILPL")   ;UT command thick  TEL polylines
("UTTELSNG"     "C-TEL"                           "5"   "BLDG")     ;UT command single line TEL lines
("UTWATOD"      "C-WATR-OD~~"                     "3"   "")    ;UT command thick water OD lines
("UTWATPL"      "C-WATR-INNR"                     "9"   "UTILPL")   ;UT command thick water polylines
("UTWATSNG"     "C-WATR"                          "3"   "")    ;UT command single line water lines
("UTXCATVOD"    "C-CATV-OD~~-E"                   "9"   "")         ;UT command thick existing CATV OD lines
("UTXCATVPL"    "C-CATV-INNR-E"                   "9"   "DOT")      ;UT command thick existing CATV polylines
("UTXCATVSNG"   "C-CATV-E"                        "9"   "")         ;UT command single line existing CATV lines
("UTXELECOD"    "C-ELEC-OD~~-E"                   "9"   "")         ;UT command thick existing ELEC OD lines
("UTXELECPL"    "C-ELEC-INNR-E"                   "9"   "DOT")      ;UT command thick existing ELEC polylines
("UTXELECSNG"   "C-ELEC-E"                        "9"   "BLDG")     ;UT command single line existing ELEC lines
("UTXGASOD"     "C-NGAS-OD~~-E"                   "9"   "")         ;UT command thick existing GAS OD lines
("UTXGASPL"     "C-NGAS-INNR-E"                   "9"   "DOT")      ;UT command thick existing GAS polylines
("UTXGASSNG"    "C-NGAS-E"                        "9"   "BLDG")     ;UT command single line existing GAS lines
("UTXIRROD"     "C-IRRG-OD~~-E"                   "9"   "")         ;UT command thick existing IRR OD lines
("UTXIRRPL"     "C-IRRG-INNR-E"                   "9"   "DOT")      ;UT command thick existing IRR polylines
("UTXIRRSNG"    "C-IRRG-E"                        "9"   "BLDG")     ;UT command single line existing IRR lines
("UTXSDOD"      "C-STRM-OD~~-E"                   "9"   "")         ;UT command thick existing SD OD lines
("UTXSDPL"      "C-STRM-INNR-E"                   "9"   "DOT")      ;UT command thick existing SD line polylines
("UTXSDSNG"     "C-STRM-E"                        "9"   "HIDDEN")   ;UT command existing single SD lines
("UTXSEWOD"     "C-SEWR-OD~~-E"                   "9"   "")         ;UT command thick existing sewer OD lines
("UTXSEWPL"     "C-SEWR-INNR-E"                   "9"   "DOT")      ;UT command thick existing sewer polylines
("UTXSEWSNG"    "C-SEWR-E"                        "9"   "")         ;UT command single line existing sewer lines
("UTXTELOD"     "C-TELE-OD~~-E"                   "9"   "")         ;UT command thick existing TEL OD lines
("UTXTELPL"     "C-TELE-INNR-E"                   "9"   "DOT")      ;UT command thick existing  TEL polylines
("UTXTELSNG"    "C-TELE-E"                        "9"   "BLDG")     ;UT command single line existing TEL lines
("UTXWATOD"     "C-WATR-OD~~-E"                   "9"   "")         ;UT command thick existing water OD lines
("UTXWATPL"     "C-WATR-INNR-E"                   "9"   "DOT")      ;UT command thick existing water polylines
("UTXWATSNG"    "C-WATR-E"                        "9"   "")    ;UT command single line existing water lines
("WALLEDGE"     "C-WALL"                          "7"   "")         ;WALL command outside edge
("WALLPL"       "C-WALL-PL"                       "7"   "DOT")      ;WALL command pline
("WALLXEDGE"    "C-WALL-E"                        "10"  "")         ;WALL command existing outside edge
("WALLXPL"      "C-WALL-INNR-E"                   "10"  "DOT")      ;WALL command existing pline
("WATSER"       "C-WATR-SERV"                     "3"   "")    ;WS command water service lines
("WATSERTX"     "C-WATR-SERV-DIM"                 "5"   "")         ;WS command water service labels
("XDIM"         "C-ANNO-DIMS-E"                   "9"   "")         ;STDIM command
